1.
В панели адреса в своём браузере вводим ip – 192.168.1.1 и нажимаем enter
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2.
В появившемся окне вводим логин и пароль (поумолчаниа admin).
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3.
В появившемся окне нажимаем WAN.
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4.
Нажимаем edit.
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5.
Ничего не меняем, нажимаем next. 
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6.
Ставим флажек на Bridging и нажимаем next.
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7.
Ничего не меняем, нажимаем next. 
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8.
Нажимаем save
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9.
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После чего перезапускаем  модем  и  создаем подключение к  интернету  на компьютере.
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WAN Setup - Summary
Make sure that the settings below match the settings provided by your ISP.

[PORT / VP / VCE: [0/8/ 35
| Connection Type: [8ridge

Service Name: _[pppoe 0.8 35 1
Service Category: [UER

Not Appicable
[Enabled
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Not Appicable
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Cick "Save” to save these settings. Click "Back” to make any modifications.
NOTE: You need to reboot to activate this WAN interface and further configure services over this interface.
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Wide Area Network (WAN) Setup

Choose Add, Ed, or Remove to configure WAN nterfaces.
Choose Save/Reboot to apply the changes and reboot the system.
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DSL Router Reboot
‘The DSL Router has been configured and is rebooting,

Close the DSL Router Configuration window and wait for 2 mimites before reopening your web browser. I necessary, reconfigure your PC's IP address to match your new configuration.
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Wide Area Network (WAN) Setup

Choose Add, Ed, or Remove to configure WAN nterfaces.
Choose Save/Reboot to apply the changes and reboot the system.
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AATM PVC Configuration
‘This screen alows you to configure an ATM PVC identfier (PORT and VPT and VCI) and select 2 service category. Othenwise choose

sor0a 0]
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Enabling packet level QoS for a PVC improves performance for selected casses of appiications. QoS cannot be set for CBR and Realt
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Connection Type

Select the type of network protocol for IP over Ethemet as WAN interface.
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